**KPN-2**

The KPN-2 is a waterproof dual relay access control unit with integrated keypad and card/fob reader. Two relays make it ideal for switching a main gate & pedestrian gate.

It is suitable for mounting either indoors or outdoors in harsh environments. It is housed in a strong, sturdy and vandal proof zinc alloy powder coated case.

This unit supports up to 999 users in multiple access configurations (card only, PIN only, or card + PIN). Both relays can operate in pulse mode (1-300 seconds) or toggle mode.

* ****Supports wide voltage input 12-28Vac/dc
* Waterproof, conforms to IP66
* Strong zinc alloy powder coated anti-vandal case
* Card frequency: 125KHz EM
* Read range: 1-6cm
* All metal keys
* Full programming from the keypad
* 2 relays
* 999 users, supports card, PIN, or card + PIN
* PIN length 1-8 digits
* Backlit keys, set always on, always off, or automatically off after 60 seconds
* Multi-colour LED status display
* Integrated alarm and buzzer output, can set volume level 0 - 5
* Pulse or toggle mode
* Built in light dependent resistor (LDR) for anti-tamper
* Pre-wired with 1 metre of cable
* Dimensions: 134 x 55.5 x 21mm
* Operating temperature: -40 to 60⁰C

Accessories:

PCARD

PFOB-IP

PFOB-G